**Additional equipment**

**Fire Protection - Stacking door MATADOOR**

**EI2 30 C2 Sa / EI2 90 C2 Sa / EI2 120 C2 Sa**

Surface coating:
Wet coating - color hues according to RAL, DB or NCS

Electrical options:
Self-holding (pulse control) with additional safety equipment possible, timed closing

Smoke switches:
Also available in RAL coated version and flush-mounted version

for suspended ceilings and false ceilings (also coated)

Command devices:
Key switch, triple push-button, radio, pull switch,

Release buttons:
Surface-mounted underglass with reset, flush-mounted underglass with reset

Other high quality push-button/reset combinations (incl. stainless steel etc.) possible on request

Automated guided vehicle systems (AGVS):
Automated (driverless) transport systems also possible with special controls